
Walking/Working Surface Safety Audit

This audit is to be completed on at least a monthly basis. All “NO” answers must be addressed through some positive action toward correction.

	General Conditions

	Yes
	No
	Inspection Point

	☐	☐	1. Are all worksites clean and orderly?

	
	If No: Identify Locations/
Department(s)
	

	
	Assigned To:
	
	Date Completed
	

	☐	☐	2. Are machines and work areas swept clean at the end of each shift or workday and are debris, scrap, and other waste picked up and removed from the work area?

	
	If No: Identify Locations/
Department(s)
	

	
	Assigned To:
	
	Date Completed
	

	☐	☐	3. Are work areas adequately illuminated?

	
	If No: Identify Locations/
Department(s)
	

	
	Assigned To:
	
	Date Completed
	

	Walkways

	Yes
	No
	Inspection Point

	☐	☐	4. Are aisles and passageways kept clear and passable?

	
	If “No” 
Note Location(s)
	
	Follow up:
	

	☐	☐	5. Are aisles and walkways marked as required?

	
	If “No” 
Note Location(s)
	
	Follow Up:
	

	☐	☐	6. Are working surfaces kept dry and free of wet or otherwise slippery conditions?

	
	If “No” 
Note Location(s)
	
	Follow Up:
	

	☐	☐	7. Are wet or slippery surfaces, inherent to the production operation, covered with non-slip material or otherwise made safe?

	
	If “No” 
Note Location(s)
	
	Follow Up:
	

	☐	☐	8. Is there safe clearance for walking in aisles where motorized equipment is used?

	
	If “No” 
Note Location(s)
	
	Follow Up:
	

	☐	☐	9. Are standard guardrails (42” high with a 21” mid rail and 4” toe board) provided whenever aisles, walkways, or working surfaces are elevated more than 4 feet off the floor or work area?

	
	If “No” 
Note Location(s)
	
	Follow Up:
	

	☐	☐	10. Are crossover points provided over conveyors or similar hazards at strategic locations to prevent people from crawling over or onto conveyor systems or similar hazards?

	
	If “No” 
Note Location(s)
	
	Follow Up:
	




	Floor Or Wall Openings

	Yes
	No
	Inspection Point

	☐	☐	11. Does a cover, guardrail, or equivalent provide protection on all sides of floor openings?

	
	If “No” 
Note Location(s)
	
	Follow Up:
	

	☐	☐	12. Are toe boards installed around the edges of permanent floor openings?

	
	If “No” 
Note Location(s)
	
	Follow Up:
	

	☐	☐	13. Are grates or similar type covers over floor openings designed so foot traffic or rolling equipment will not be affected by the spacing or construction of the grate?

	
	If “No” 
Note Location(s)
	
	Follow Up:
	

	☐	☐	14. Are unused portions of service pits and pits not actually in use either covered or protected by guardrails or equivalent?

	
	If “No” 
Note Location(s)
	
	Follow Up:
	

	Stairs and Stairways

	Yes
	No
	Inspection Point

	☐	☐	Are standard stair rails or handrails on all stairways having four or more risers (steps)?

	
	

	☐	☐	Are all stairways at least 22” wide?

	
	

	☐	☐	Is there a vertical clearance of at least 7 feet from the leading edge of any stair tread to any overhead obstruction, which also includes the ceiling?

	
	

	☐	☐	Are all step risers on stairs uniform in height from top to bottom?

	
	

	☐	☐	Are steps on stairs and stairways designed or provided with a surface that renders them slip-resistant?

	
	

	☐	☐	Are stairway handrails located between 30-34” above the leading edge of the stair treads?

	
	

	☐	☐	Do stairway handrails have at least 3” of clearance between the handrails and the surface they are mounted to?

	
	

	Elevated Surfaces

	Yes
	No
	Inspection Point

	
	
	Are surfaces elevated more than 4 feet above the floor or ground protected with standard guardrails (a railing 42” from the floor with a mid rail at 21”)?

	
	
	Are all elevated surfaces provided with a standard 4” toeboard?



Date: ____________
Completed By: __________________
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