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Property Protection Safety Survey                           Date:  _______    Location: ______________
Property Protection Survey (Fire)

	Facility Name:
	Date:

	Address:
	City:

	Inspector:
	Title: 



	1
	BUILDING GROUNDS

	1.1
	Is there adequate clearance from tree branches/canopies to building structure?
	☐ Yes
	☐ No

	1.2
	Are gutters and roofs free of accumulated pine needles and leaves?
	☐ Yes
	☐ No

	1.3
	Are there designated areas for smoking with proper extinguishing containers?
	☐ Yes
	☐ No

	1.4
	Trash receptacles less than 40 gallons are constructed of non-combustible materials.
	☐ Yes
	☐ No

	1.5
	Trash receptacles are not overflowing and located 20 feet from the building
	☐ Yes
	☐ No

	1.6
	Combustible material is not stored within 10 feet of any building or structure
	☐ Yes
	☐ No

	1.7
	A firebreak is maintained at least 30 feet on each side of the property line – all flammable vegetation or other combustible growth. (Does not include shrubbery or plants used as ground cover)
	☐ Yes
	☐ No

	1.8
	Fire lanes marked “Fire Lane No Parking” and clearly visible
	☐ Yes
	☐ No

	☐	List Deficiency Location(s):

	☐	Corrective Action:
	Assigned To: 
	Complete By:
	Completed:

	☐	List Deficiency Location(s):

	☐	Corrective Action:
	Assigned To:
	Complete By:
	Completed:




	2
	COMPRESSED GAS CYLINDERS

	2.1
	Are compressed gas cylinders stored in well-ventilated area, away from source of ignition?
	☐ Yes
	☐ No

	2.2
	Are cylinders legibly marked with proper hazardous symbol to clearly identify the gas contained?
	☐ Yes
	☐ No

	2.3
	Are cylinders secured to a wall or dolly at one-third and two-thirds the height?
	☐ Yes
	☐ No

	2.4
	Combustible and flammable materials kept 20 feet from all cylinders?
	☐ Yes
	☐ No

	2.5
	No Smoking signs are posted near cylinders?
	☐ Yes
	☐ No

	2.6
	Oxygen and fuel-gas cylinders are segregated by 20 feet or 5 feet non-combustible barrier?
	☐ Yes
	☐ No

	2.7
	LPG cylinders are not stored inside buildings?
	☐ Yes
	☐ No

	2.8
	Are cylinder caps installed on cylinders that are not in use?
	☐ Yes
	☐ No

	☐	List Deficiency Location(s):

	☐	Corrective Action:
	Assigned To:
	Complete By:
	Completed:

	☐	List Deficiency Location(s):

	☐	Corrective Action:
	Assigned To:
	Complete By:
	Completed:
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	ELECTRICAL EQUIPMENT

	3.1
	Temporary wiring (extension cords) is not used more than 90 days. 
	☐ Yes
	☐ No

	3.2
	Where temporary wiring is used, should a work order be placed to install additional electrical source?
	☐ Yes
	☐ No

	3.3
	All outlets and electrical enclosures have plates/covers and in good condition.
	☐ Yes
	☐ No

	3.4
	Only one surge protector is plugged directly into the wall (no extension cords).
	☐ Yes
	☐ No

	3.5
	Access to breaker control panels if free of obstructions (30” clearance all around)
	☐ Yes
	☐ No

	3.6
	Are all circuit breakers within electrical panels clearly labeled (no open spaces present)?
	☐ Yes
	☐ No

	3.7
	*Portable heaters are listed by Underwriters’ Laboratories, equipped with automatic shut off feature and kept 3 feet from flammable/combustible material. (*Unless heaters are prohibited by the AHJ.)
	☐ Yes
	☐ No

	3.8
	Have Arc Flash warning labels been placed on electrical control panels and clearly state appropriate PPE, boundaries, etc.  
	☐ Yes
	☐ No

	☐	List Deficiency Location(s):

	☐	Corrective Action:
	Assigned To:
	Complete By:
	Completed:
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	EXIT DOORS/EGRESS

	4.1
	Are exit signs visible and illuminated?
	☐ Yes
	☐ No

	4.2
	Have exit signs and emergency lighting been tested and are they functioning properly?
	☐ Yes
	☐ No

	4.3
	Are exit paths, including stairwells and doors free from obstructions?
	☐ Yes
	☐ No

	4.4
	Are adjacent doors, passageways or stairways leading to rooms or areas that are not part of the exit or lead to a dead end hallway identified and marked “NOT AN EXIT”?
	☐ Yes
	☐ No

	4.5
	Evacuation plans are posted where appropriate?
	☐ Yes
	☐ No

	4.6
	Can exit doors open from direction of travel without use of a key or any special knowledge or effort?
	☐ Yes
	☐ No

	4.7
	Are exit doors equipped with panic hardware and able to open with a force of 15 pounds or less?
	☐ Yes
	☐ No

	4.8
	Are self-closing fire rated doors free from impairment (propped open, blocked) and functioning properly?
	☐ Yes
	☐ No

	4.9
	Have fire rated doors been compromised to include installation of windows or other alterations that were not part of the door’s original design and impacts the doors fire rating and integrity?
	☐ Yes
	☐ No

	4.10
	Are fire rated doors properly and visibly labeled?
	☐ Yes
	☐ No

	4.11
	Are fire rated doors free from obstructions preventing them from automatically closing?
	☐ Yes
	☐ No




4 Exit Doors/Egress (Continued)
	☐	List Deficiency Location(s):

	☐	Corrective Action:
	Assigned To:
	Complete By:
	Completed:



	☐	List Deficiency Location(s):

	☐	Corrective Action:
	Assigned To:
	Complete By:
	Completed:
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	FIRE PROTECTION

	5.1
	Has the fire alarm been tested within the past 12 months by a properly trained and competent person? 
	☐ Yes
	☐ No

	5.2
	Have the fire doors been inspected within the last 30 days?
	☐ Yes
	☐ No

	5.3
	Have fire doors had a “drop” test within the past 12 months?
	☐ Yes
	☐ No

	5.4
	Has automatic sprinkler system been inspected and tested quarterly and annually by a qualified contractor?
	☐ Yes
	☐ No

	5.5
	Is there an adequate representation of spare sprinkler heads and a spanner wrench located near the fire sprinkler riser?
	☐ Yes
	☐ No

	5.6
	Are post indicator valves (PIV) “spring” test conducted on a monthly basis and do the valves indicate that they are in the open position?
	☐ Yes
	☐ No

	5.7
	Are fire pump 30-minute churn test conducted weekly?
	☐ Yes
	☐ No

	5.8
	Are backup generator(s) and power supply on automatic start up weekly for 30 minutes 
	☐ Yes
	☐ No

	5.9
	Are automatic sprinkler system water control valves, air and water pressure checked weekly (or as required by AHJ)?
	☐ Yes
	☐ No

	5.10
	Has the fire sprinkler system been certified within the past (5) years by a contractor qualified by the State of California?
	☐ Yes
	☐ No

	5.11
	Are Fire Department Connection (FDC) caps in place? 
	☐ Yes
	☐ No

	5.12
	Are Fire Sprinkler control valves physically locked in the open position with a chain and breakable lock and electronically supervised by the alarm company?
	☐ Yes
	☐ No

	5.13
	Are portable fire extinguishers mounted and charged at appropriate exits and not more than 75’ distance between extinguishers?
	☐ Yes
	☐ No

	5.14
	Are portable fire extinguishers inspected and recharged within the past 12 months?
	☐ Yes
	☐ No

	5.15
	Are portable fire extinguishers checked monthly and recorded?
	☐ Yes
	☐ No

	5.16
	Are fire extinguishers visible (no obstructions within 3 feet)?
	☐ Yes
	☐ No

	5.17
	Sprinkler heads have 18 inches of clearance (bottom of head to nearest vertical object)?
	☐ Yes
	☐ No

	5.18
	All ceiling tiles are in place and there are no openings in attic space or area above ceiling.
	☐ Yes
	☐ No

	5.19
	Do all recessed sprinkler heads have escutcheon rings?
	☐ Yes
	☐ No





5 Fire Protection (Continued)
	☐	List Deficiency Location(s):

	☐	Corrective Action: 
	Assigned To:
	Complete By:
	Completed

	☐	List Deficiency Location(s):

	☐	Corrective Action: 
	Assigned To:
	Complete By:
	Completed
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	FLAMMABLE AND COMBUSTIBLE MATERIALS

	6.1
	Are wood pallets, flammable debris and waste materials stored at least 20 feet from buildings?
	☐ Yes
	☐ No

	6.2
	Wood dust and shavings vacuumed daily in woodshops?
	☐ Yes
	☐ No

	6.3
	Are flammable liquids and aerosols stored in an Underwriters’ Laboratory listed or Factory Mutual approved flammable storage cabinet?
	☐ Yes
	☐ No

	6.4
	Are less than 60 gallons of flammable liquids in a single flammable liquids storage cabinet?
	☐ Yes
	☐ No

	6.5
	Are there no more than three (3) storage cabinets in a single storage area?
	☐ Yes
	☐ No

	6.6
	Are flammable liquid storage cabinets free of normal combustible materials such as paper, and cardboard?
	☐ Yes
	☐ No

	6.7
	Do flammable liquids storage cabinets function properly to include self-closing doors and (3) point latching mechanisms?
	☐ Yes
	☐ No

	6.8
	Are approved storage cabinets labeled “Flammable-Keep Away from Open Flames”
	☐ Yes
	☐ No

	6.9
	Are all flammable liquids stored away from exits, stairways or means of travel?
	☐ Yes
	☐ No

	6.10
	Are approved safety cans or department of transportation approved containers used for handling and use of flammable liquids, quantities of 5 gallons or less?
	☐ Yes
	☐ No

	6.11
	Are oil and paint rags stored in a dedicated metal container with a self-closing lid?
	☐ Yes
	☐ No

	6.12
	There are no combustible materials (paper, hanging mobiles) on exit doors, ceilings, electrical panels, light fixtures, fire sprinklers and heaters.
	☐ Yes
	☐ No

	6.13
	Are drums used to transfer flammable liquids properly grounded and bonded?
	☐ Yes
	☐ No

	☐	List Deficiency Location(s):

	☐	Corrective Action:
	Assigned To:
	Complete By:
	Completed

	☐	List Deficiency Location(s):

	☐	Corrective Action:
	Assigned To:
	Complete By:
	Completed




	7
	KITCHEN – Fixed Extinguishing System

	7.1
	Has fixed extinguishing system been inspected/tagged within the past 6 months?
	☐ Yes
	☐ No

	7.2
	Are fire control manual (pull) releases visible?
	☐ Yes
	☐ No

	7.3
	Are all filters in place and installed vertically?
	
	

	7.4
	Are hoods, filters, vents, and fans maintained free of grease and serviced at regular intervals?
(Quarterly-high-volume cooking operations; Semi-Annually - moderate volume cooking; Annually-low-volume cooking operations)
	☐ Yes
	☐ No

	7.5
	Are caps firmly attached to extinguishing nozzles?
	☐ Yes
	☐ No

	7.6
	Is there a 16-inch separation between the fryer and open flame?
	☐ Yes
	☐ No

	7.7
	If “No” to 7.6 – Is a steel or tempered glass baffle plate installed at 8-inch minimum height between the fryer and surface flames of adjacent appliance?
	☐ Yes
	☐ N/A


	☐	List Deficiency Location(s):

	☐	Corrective Action:
	Assigned To:
	Complete By:
	Completed:

	☐	List Deficiency Location(s):

	☐	Corrective Action:
	Assigned To:
	Complete By:
	Completed:
















Updated:  9/2025

This Alliant Risk Control Consulting checklist is not intended to be exhaustive. The discussion and best practices suggested herein should not be regarded as legal advice.  
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