Walking/Working Surface Safety Audit


	Department:
	
	Location:
	
	Date:
	

	Completed By:
	
	
	
	
	


								
	General Conditions

	Yes
	No
	Inspection Point

	
	
	A. Are all worksites clean and orderly?

	
	
	B. Are machines and work areas swept clean at the end of each shift or workday and are debris, scrap, and other waste picked up and removed from the work area?

	
	
	C. Are work areas adequately illuminated?

	Walkways

	Yes
	No
	Inspection Point

	
	
	D. Are aisles and passageways kept clear and passable?

	
	
	E. Are aisles and walkways marked as required?

	
	
	F. Are working surfaces kept dry and free of wet or otherwise slippery conditions?

	
	
	G. Are wet or slippery surfaces, inherent to the production operation, covered with non-slip material or otherwise made safe?

	
	
	H. Is there safe clearance for walking in aisles where motorized equipment is used?

	
	
	I. Are standard guardrails (42” high with a 21” mid rail and 4” toeboard) provided whenever aisles, walkways, or working surfaces are elevated more than 4 feet off the floor or work area?

	
	
	J. Are bridges or crossovers provided over conveyors or similar hazards at strategic locations to prevent people from crawling over or onto conveyor systems or similar hazards?

	Floor Or Wall Openings

	Yes
	No
	Inspection Point

	
	
	K. Does a cover, guardrail, or equivalent provide protection on all sides of floor openings?

	
	
	L. Are toeboards installed around the edges of permanent floor openings?

	
	
	M. Are grates or similar type covers over floor openings designed so foot traffic or rolling equipment will not be affected by the spacing or construction of the grate?

	
	
	N. Are unused portions of service pits and pits not actually in use either covered or protected by guardrails or equivalent?

	Stairs and Stairways

	Yes
	No
	Inspection Point

	
	
	O. Are standard stair rails or handrails on all stairways having four or more risers (steps)?

	
	
	P. Are all stairways at least 22” wide?

	
	
	Q. Is there a vertical clearance of at least 7 feet from the leading edge of any stair tread to any overhead obstruction, which also includes the ceiling?

	
	
	R. Are all step risers on stairs uniform in height from top to bottom?

	
	
	S. Are steps on stairs and stairways designed or provided with a surface that renders them slip-resistant?

	
	
	T. Are stairway handrails located between 30-34” above the leading edge of the stair treads?

	
	
	U. Do stairway handrails have at least 3” of clearance between the handrails and the surface they are mounted to?

	Elevated Surfaces

	Yes
	No
	Inspection Point

	
	
	V. Are surfaces elevated more than 4 feet above the floor or ground protected with standard guardrails (a railing 42” from the floor with a mid rail at 21”)?

	
	
	W. Are all elevated surfaces provided with a standard 4” toeboard?



Date: ____________
Completed By: __________________

	ITEM
	CORRECTIVE ACTION
	ASSIGNED TO
	COMPLETED

	
	
	
	

	
	
	
	

	
	
	
	

	
	
	
	



This audit is to be completed on at least a monthly basis. All “NO” answers must be addressed with a corrective action with a completion date.
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